Correction Annex for Jufeng Cableway Equipment Upgrade Project

1. Original Bidding Documents: 1.2.2.5.2.5.1 Horizontally moving 8-passenger gondolas shall be used, and each gondola shall be able to accommodate eight passengers."

**Changed to:** 1.2.2.5.2.5.1 Horizontally moving 8-passenger gondolas shall be used, and each gondola shall be able to accommodate eight passengers (the number of passengers may be reduced for glass-bottom gondolas)

2. Original Bidding Documents: 1.2.2.5.2.10.6 Sheave release switches on the trestles. Sheave release protection switches, rope position detection systems and dual safety wires shall be provided on the trestles as needed, with each trestle having an independent safety circuit."

**Changed to:** 1.2.2.5.2.10.6 Sheave release switches on the trestles. Sheave release protection switches shall be provided on the trestles as needed, with each trestle having an independent safety circuit.

3. Original Bidding Documents: 1.2.2.5.2.12 Spare parts

The Bidder must provide a detailed list of spare parts that meet the following requirements:

1.2.2.5.2.12.1 Sufficient mechanical spare parts for two years of operation. (List attached hereinafter)

1.2.2.5.2.12.2 Sufficient electrical spare parts for two years of operation. (List attached hereinafter)

List of Spare Parts

(Including but not limited to the items listed in the table, but at least including the listed spare parts (matching the submitted equipment). The Bidders may add additional items at their discretion.

**Changed to:** 1.2.2.5.2.12 Spare parts

In the Bid, the Bidder must provide a detailed list of spare parts that meet the following requirements:

1.2.2.5.2.12.1 Sufficient mechanical spare parts for two years of operation.

1.2.2.5.2.12.2 Sufficient electrical spare parts for two years of operation.

4. Original Bidding Documents: 1.2.2.7.2 Hydraulic motors, diesel fuel tanks, pipelines and hydraulic fuel tanks must be equipped with heating functions."

**Changed to:** 1.2.2.7.2 Diesel engine diesel fuel tanks, pipelines, etc. must be equipped with heating functions. The hydraulic system must be capable of normal operation at temperatures below -30°C.

5. Original Bidding Documents: 1.2.2.5.2.3.2 The hydraulic cylinders shall have an effective stroke of not less than 5 meters."

**Changed to:** 1.2.2.5.2.3.2 The hydraulic tensioning system shall have a total effective stroke of not less than 5 meters.

6. Original Bidding Documents: Chapter V Invitation for Bids, Chapter VI Bid Data Sheet, and the Annex I Stage I Conformity Checklist: "The equipment submitted should be mature and reliable, and must possess the "Manufacture License of Special Equipment of the People's Republic of China" issued by the State Administration for Market Regulation, or provide relevant supporting documents for the registration of imported passenger ropeway products".

**Changed to:** Chapter V Invitation for Bids, Chapter VI Bid Data Sheet, and the Annex I Stage I Conformity Checklist: "The equipment submitted should be mature and reliable, and must possess the "Manufacture License of Special Equipment of the People's Republic of China" issued by the State Administration for Market Regulation, or provide relevant supporting documents for the registration of imported passenger ropeway products, or provide special equipment type test reports and certificate of conformity for special equipment type test."

7. Original Bidding Documents: "Annex II Commercial Evaluation Form

1. If the bid product passes the ISO 3834 International Welding Quality System Certification, there will be one point;

2. If the bid product passes the OHSAS 18001 Occupational Health and Safety Management System Certification, there will be one point.

Note: Please provide a copy (Chinese translation is required for foreign documents) in the Bid; otherwise there will be no points."

**Changed to:** "1. If the bid product passes the ISO 3834 International Welding Quality System Certification or EN1090 Certification, there will be one point;

2. If the bid product passes the OHSAS 18001 Occupational Health and Safety Management System Certification or ISO45001:2018 Management System Certification, there will be one point.

Note: Please provide a copy (Chinese translation is required for foreign documents) in the Bid; otherwise there will be no points."

8. Original Bidding Documents: "Annex II Commercial Evaluation Form: According to the performance of the detachable ropeway that has been accepted and put into operation by the cable inspection center before the bid opening, there will be additional 0.5 points for each ropeway, up to a maximum of two points. (The number of Passenger Ropeway Safety Inspection Certificates issued by the State Administration for Market Regulation shall prevail.)

(Fill in the explanation in Annex 7 "List of Implementation of Similar Projects by Bidders" in the Commercial Part of the Bid)"

**Changed to:** "Annex II Commercial Evaluation Form: According to the performance of the detachable ropeway that has been accepted and put into operation by the cable inspection center before the bid opening, there will be additional 0.5 points for each ropeway, up to a maximum of two points. (The number of Passenger Ropeway Safety Inspection Certificates issued by the State Administration for Market Regulation shall prevail.)

(Fill in the explanation in "List of Implementation of Similar Projects by Bidders" in the Commercial Part of the Bid, with the format to be determined by the bidder and without starting time limit.")